#!C:\mtkclient-main\python.exe
# MTK Stage2 Client (c) B.Kerler 2018-2021.
# Licensed under MIT License

import os
import sys
import logging
import time
import argparse
import hashlib
from binascii import hexlify
from struct import pack, unpack
from mtkclient.Library.usblib import usb_class
from mtkclient.Library.utils import LogBase
from mtkclient.Library.utils import print_progress
from mtkclient.Library.hwcrypto import crypto_setup, hwcrypto
from mtkclient.config.brom_config import Mtk_Config
from mtkclient.config.usb_ids import default_ids

class Stage2(metaclass=LogBase):
    def __init__(self, args, loglevel=logging.INFO):
        self.__logger = self.__logger
        self.args = args
        self.loglevel = loglevel
        self.info = self.__logger.info
        self.error = self.__logger.error
        self.warning = self.__logger.warning
        self.emmc_inited = False
        # Setup HW Crypto chip variables
        self.setup = crypto_setup()

        if loglevel == logging.DEBUG:
            logfilename = os.path.join("logs", "log.txt")
            if os.path.exists(logfilename):
                os.remove(logfilename)
            fh = logging.FileHandler(logfilename)
            self.__logger.addHandler(fh)
            self.__logger.setLevel(logging.DEBUG)
        else:
            self.__logger.setLevel(logging.INFO)

        self.cdc = usb_class(portconfig=default_ids, loglevel=loglevel, devclass=10)
        self.usbread=self.cdc.usbread
        self.usbwrite=self.cdc.usbwrite

    def preinit(self):
        try:
            hwcode = self.read32(0x8000000)
        except:
            print("Error reading hwcode...aborting.")
            return False
        self.config = Mtk_Config(self.loglevel)
        self.config.init_hwcode(hwcode)
        self.setup.blacklist = self.config.chipconfig.blacklist
        self.setup.gcpu_base = self.config.chipconfig.gcpu_base
        self.setup.dxcc_base = self.config.chipconfig.dxcc_base
        self.setup.da_payload_addr = self.config.chipconfig.da_payload_addr
        self.setup.sej_base = self.config.chipconfig.sej_base
        self.setup.read32 = self.read32
        self.setup.write32 = self.write32
        self.setup.writemem = self.memwrite
        self.setup.meid_addr = self.config.chipconfig.meid_addr
        self.setup.socid_addr = self.config.chipconfig.socid_addr
        self.hwcrypto = hwcrypto(self.setup, self.loglevel)
        return True

    def init_emmc(self):
        self.usbwrite(pack(">I", 0xf00dd00d))
        self.usbwrite(pack(">I", 0x6001))
        if unpack("<I", self.usbread(4))[0] != 0x1:
            self.usbwrite(pack(">I", 0xf00dd00d))
            self.usbwrite(pack(">I", 0x6000))
            time.sleep(2)
            if unpack("<I", self.usbread(4))[0] == 0xD1D1D1D1:
                return True
            self.emmc_inited = True
        return False

    def jump(self, addr):
        self.usbwrite(pack(">I", 0xf00dd00d))
        self.usbwrite(pack(">I", 0x4001))
        self.usbwrite(pack(">I", addr))
        time.sleep(5)
        if unpack("<I", self.usbread(4))[0] == 0xD0D0D0D0:
            return True
        return False

    def read32(self, addr, dwords=1):
        result = []
        for pos in range(dwords):
            self.usbwrite(pack(">I", 0xf00dd00d))
            self.usbwrite(pack(">I", 0x4002))
            self.usbwrite(pack(">I", addr + (pos * 4)))
            self.usbwrite(pack(">I", 4))
            result.append(unpack("<I", self.usbread(4))[0])
        if len(result) == 1:
            return result[0]
        return result

    def cmd_C8(self, val) -> bool:
        'Clear cache func'
        self.usbwrite(pack(">I", 0xf00dd00d))
        self.usbwrite(pack(">I", 0x5000))
        ack = self.usbread(4)
        if ack == b"\xD0\xD0\xD0\xD0":
            return True
        return False

    def write32(self, addr, dwords) -> bool:
        if isinstance(dwords, int):
            dwords = [dwords]
        for pos in range(0, len(dwords)):
            self.usbwrite(pack(">I", 0xf00dd00d))
            self.usbwrite(pack(">I", 0x4000))
            self.usbwrite(pack(">I", addr + (pos * 4)))
            self.usbwrite(pack(">I", 4))
            self.usbwrite(pack("<I", dwords[pos]))
            ack = self.usbread(4)
            if ack == b"\xD0\xD0\xD0\xD0":
                continue
            else:
                return False
        return True

    def connect(self):
        self.cdc.connected = self.cdc.connect()
        return self.cdc.connected

    def close(self):
        if self.cdc.connected:
            self.cdc.close()

    def readflash(self, type: int, start, length, display=False, filename: str = None):
        if not self.emmc_inited:
            self.init_emmc()
        wf = None
        buffer = bytearray()
        if filename is not None:
            wf = open(filename, "wb")
        sectors = (length // 0x200)
        sectors += (1 if length % 0x200 else 0)
        startsector = (start // 0x200)
        # emmc_switch(1)
        self.usbwrite(pack(">I", 0xf00dd00d))
        self.usbwrite(pack(">I", 0x1002))
        self.usbwrite(pack(">I", type))

        if display:
            print_progress(0, 100, prefix='Progress:', suffix='Complete', bar_length=50)

        # kick-wdt
        # self.usbwrite(pack(">I", 0xf00dd00d))
        # self.usbwrite(pack(">I", 0x3001))

        bytestoread = length
        bytesread = 0
        old = 0
        # emmc_read(0)
        for sector in range(startsector, sectors):
            self.usbwrite(pack(">I", 0xf00dd00d))
            self.usbwrite(pack(">I", 0x1000))
            self.usbwrite(pack(">I", sector))
            tmp = self.usbread(0x200)
            if not tmp or len(tmp) != 0x200:
                self.error("Error on getting data")
                return
            if display:
                prog = sector / sectors * 100
                if round(prog, 1) > old:
                    print_progress(prog, 100, prefix='Progress:',
                                   suffix='Complete, Sector:' + hex(sector),
                                   bar_length=50)
                    old = round(prog, 1)
            bytesread += len(tmp)
            size = min(bytestoread, len(tmp))
            if wf is not None:
                wf.write(tmp[:size])
            else:
                buffer.extend(tmp)
            bytestoread -= size
        if display:
            print_progress(100, 100, prefix='Complete: ', suffix=filename, bar_length=50)
        if wf is not None:
            wf.close()
        else:
            return buffer[start % 0x200:(start % 0x200) + length]

    def preloader(self, start, length, filename):
        sectors = 0
        if start != 0:
            start = (start // 0x200)
        if length != 0:
            sectors = (length // 0x200) + (1 if length % 0x200 else 0)
        self.info("Reading preloader...")
        if self.cdc.connected:
            if sectors == 0:
                buffer = self.readflash(type=1, start=0, length=0x4000, display=False)
                if len(buffer) != 0x4000:
                    print("Error on reading boot1 area.")
                    return
                if buffer[:9] == b'EMMC_BOOT':
                    startbrlyt = unpack("<I", buffer[0x10:0x14])[0]
                    if buffer[startbrlyt:startbrlyt + 5] == b"BRLYT":
                        start = unpack("<I", buffer[startbrlyt + 0xC:startbrlyt + 0xC + 4])[0]
                        st = buffer[start:start + 4]
                        if st == b"MMM\x01":
                            length = unpack("<I", buffer[start + 0x20:start + 0x24])[0]
                            data = self.readflash(type=1, start=0, length=start + length, display=True)
                            if len(data) != start + length:
                                print("Warning, please rerun command, length doesn't match.")
                            idx = data.find(b"MTK_BLOADER_INFO")
                            if idx != -1:
                                filename = data[idx + 0x1B:idx + 0x3D].rstrip(b"\x00").decode('utf-8')
                            with open(os.path.join("logs", filename), "wb") as wf:
                                wf.write(data[start:start + length])
                                print("Done writing to " + os.path.join("logs", filename))
                            with open(os.path.join("logs", "hdr_" + filename), "wb") as wf:
                                wf.write(data[:start])
                                print("Done writing to " + os.path.join("logs", "hdr_" + filename))

                            return
                else:
                    length = 0x40000
                    self.readflash(type=1, start=0, length=length, display=True, filename=filename)
                    print("Done")
                print("Error on getting preloader info, aborting.")
            else:
                self.readflash(type=1, start=start, length=length, display=True, filename=filename)
            print("Done")

    def boot2(self, start, length, filename):
        sectors = 0
        if start != 0:
            start = (start // 0x200)
        if length != 0:
            sectors = (length // 0x200) + (1 if length % 0x200 else 0)
        self.info("Reading boot2...")
        if self.cdc.connected:
            if sectors == 0:
                self.readflash(type=2, start=0, length=0x40000, display=True, filename=filename)
                print("Done")
            else:
                self.readflash(type=1, start=start, length=length, display=True, filename=filename)
            print("Done")

    def memread(self, start, length, filename=None):
        bytestoread = length
        addr = start
        data = b""
        pos = 0
        if filename is not None:
            wf = open(filename, "wb")
        while bytestoread > 0:
            size = min(bytestoread, 0x100)
            self.usbwrite(pack(">I", 0xf00dd00d))
            self.usbwrite(pack(">I", 0x4002))
            self.usbwrite(pack(">I", addr + pos))
            self.usbwrite(pack(">I", size))
            if filename is None:
                data += self.usbread(size)
            else:
                wf.write(self.usbread(size))
            bytestoread -= size
            pos += size
        self.info(f"{hex(start)}: " + hexlify(data).decode('utf-8'))
        if filename is not None:
            wf.close()
        return data

    def memwrite(self, start, data, filename=None):
        if filename is not None:
            rf = open(filename, "rb")
            bytestowrite = os.stat(filename).st_size
        else:
            if isinstance(data, str):
                data = bytes.fromhex(data)
            elif isinstance(data, int):
                data = pack("<I", data)
            bytestowrite = len(data)
        addr = start
        pos = 0
        while bytestowrite > 0:
            size = min(bytestowrite, 0x100)
            self.usbwrite(pack(">I", 0xf00dd00d))
            self.usbwrite(pack(">I", 0x4000))
            self.usbwrite(pack(">I", addr + pos))
            self.usbwrite(pack(">I", size))
            if filename is None:
                wdata = data[pos:pos + size]
            else:
                wdata = rf.read(size)
            bytestowrite -= size
            pos += size
            while len(wdata) % 4 != 0:
                wdata += b"\x00"
            self.usbwrite(wdata)

        if filename is not None:
            rf.close()
        ack = self.usbread(4)
        if ack == b"\xD0\xD0\xD0\xD0":
            return True
        else:
            return False

    def rpmb(self, start, length, filename, reverse=False):
        if not self.emmc_inited:
            self.init_emmc()
        if start == 0:
            start = 0
        else:
            start = (start // 0x100)
        if length == 0:
            sectors = 4 * 1024 * 1024 // 0x100
        else:
            sectors = (length // 0x100) + (1 if length % 0x100 else 0)
        self.info("Reading rpmb...")

        self.usbwrite(pack(">I", 0xf00dd00d))
        self.usbwrite(pack(">I", 0x1002))
        self.usbwrite(pack(">I", 0x1))

        # kick-wdt
        # self.usbwrite(pack(">I", 0xf00dd00d))
        # self.usbwrite(pack(">I", 0x3001))

        print_progress(0, 100, prefix='Progress:', suffix='Complete', bar_length=50)
        bytesread = 0
        old = 0
        bytestoread = sectors * 0x100
        with open(filename, "wb") as wf:
            for sector in range(start, sectors):
                self.usbwrite(pack(">I", 0xf00dd00d))
                self.usbwrite(pack(">I", 0x2000))
                self.usbwrite(pack(">H", sector))
                tmp = self.usbread(0x100)
                if reverse:
                    tmp = tmp[::-1]
                if len(tmp) != 0x100:
                    self.error("Error on getting data")
                    return
                prog = sector / sectors * 100
                if round(prog, 1) > old:
                    print_progress(prog, 100, prefix='Progress:',
                                   suffix='Complete, Sector:' + hex((sectors * 0x200) - bytestoread),
                                   bar_length=50)
                    old = round(prog, 1)
                bytesread += 0x100
                size = min(bytestoread, len(tmp))
                wf.write(tmp[:size])
                bytestoread -= size
            print_progress(100, 100, prefix='Complete: ', suffix=filename, bar_length=50)
        print("Done")

    def keys(self, data=b"", otp=None, mode="dxcc"):
        # self.hwcrypto.disable_range_blacklist("cqdma",self.cmd_C8)
        keyinfo=""
        if self.setup.dxcc_base is not None and mode not in ["sej_aes_decrypt","sej_aes_encrypt","dxcc_sha256"]:
            rpmbkey = self.hwcrypto.aes_hwcrypt(btype="dxcc",mode="rpmb")
            rpmb2key = self.hwcrypto.aes_hwcrypt(btype="dxcc", mode="rpmb2")
            fdekey = self.hwcrypto.aes_hwcrypt(btype="dxcc",mode="fde")
            ikey = self.hwcrypto.aes_hwcrypt(btype="dxcc",mode="itrustee")
            platkey, provkey = self.hwcrypto.aes_hwcrypt(btype="dxcc",mode="prov")
            keyinfo+="\nKeys :\n-----------------------------------------\n"
            keyinfo+="RPMB:         " + hexlify(rpmbkey).decode('utf-8')+"\n"
            keyinfo+="RPMB2:         " + hexlify(rpmb2key).decode('utf-8') + "\n"
            keyinfo+="FDE :         " + hexlify(fdekey).decode('utf-8')+"\n"
            keyinfo+="iTrustee:     " + hexlify(ikey).decode('utf-8')+"\n"
            keyinfo+="Platform:     " + hexlify(platkey).decode('utf-8')+"\n"
            keyinfo+="Provisioning: " + hexlify(provkey).decode('utf-8')+"\n"
            keyinfo+="\n"
            with open(os.path.join("logs", "rpmbkey.txt"), "wb") as wf:
                wf.write(hexlify(rpmbkey))
            with open(os.path.join("logs", "rpmbkey2.txt"), "wb") as wf:
                wf.write(hexlify(rpmbkey))
            with open(os.path.join("logs", "fdekey.txt"), "wb") as wf:
                wf.write(hexlify(fdekey))
            with open(os.path.join("logs", "itrustee_fbe.txt"), "wb") as wf:
                wf.write(hexlify(ikey))
            with open(os.path.join("logs", "platkey.txt"), "wb") as wf:
                wf.write(hexlify(platkey))
            with open(os.path.join("logs", "provkey.txt"), "wb") as wf:
                wf.write(hexlify(provkey))
            return [rpmbkey, fdekey, ikey, platkey, provkey], keyinfo
        elif self.setup.sej_base is not None and mode not in ["sej_aes_decrypt","sej_aes_encrypt","dxcc_sha256"]:
            rpmbkey = self.hwcrypto.aes_hwcrypt(mode="rpmb", data=data, otp=otp, btype="sej")
            keyinfo+="\nKeys :\n-----------------------------------------\n"
            keyinfo+="RPMB: " + hexlify(rpmbkey).decode('utf-8')
            keyinfo+="\n"
            with open(os.path.join("logs", "rpmbkey.txt"), "wb") as wf:
                wf.write(hexlify(rpmbkey))
            return rpmbkey, keyinfo
        if mode == "sej_aes_decrypt":
            dec_data = self.hwcrypto.aes_hwcrypt(mode="cbc", data=data, btype="sej", encrypt=False)
            keyinfo+="\n"
            keyinfo+="Data: " + hexlify(dec_data).decode('utf-8')
            keyinfo+="\n"
            return dec_data, keyinfo
        elif mode == "sej_aes_encrypt":
            enc_data = self.hwcrypto.aes_hwcrypt(mode="cbc", data=data, btype="sej", encrypt=True)
            keyinfo+="\n"
            keyinfo+="Data: " + hexlify(enc_data).decode('utf-8')
            keyinfo+="\n"
            return enc_data, keyinfo
        elif mode == "dxcc_sha256":
            sha256val = self.hwcrypto.aes_hwcrypt(mode="sha256", data=data, btype="dxcc")
            keyinfo+="\n"
            keyinfo+="SHA256: " + hexlify(sha256val).decode('utf-8')
            keyinfo+="\n"
            return sha256val, keyinfo
        return None, ""

    def reboot(self):
        print("Rebooting..")
        self.usbwrite(pack(">I", 0xf00dd00d))
        self.usbwrite(pack(">I", 0x3000))



def getint(valuestr):
    if valuestr == '':
        return None
    try:
        return int(valuestr)
    except Exception as err:
        err = err
        try:
            return int(valuestr, 16)
        except Exception as err:
            err = err
            pass
    return 0


cmds = {
    "rpmb": 'Dump rpmb',
    "preloader": 'Dump preloader',
    "boot2": 'Dump boot2',
    "reboot": 'Reboot phone',
    "memread": "Read memory [Example: memread 0 0x10]",
    "memwrite": "Write memory [Example: memwrite 0x200000 1122334455667788, memwrite 0x0 0x12345678, " +
                "memwrite 0x0 data.bin]",
    "keys": "Extract rpmb and fde key",
    "seccfg": "Generate unlock config"
}

info = "MTK Stage2 client (c) B.Kerler 2021"


def showcommands():
    print(info)
    print("-----------------------------------\n")
    print("Available commands are:\n")
    for cmd in cmds:
        print("%20s" % (cmd) + ":\t" + cmds[cmd])
    print()


def main():
    parser = argparse.ArgumentParser(description=info)
    subparsers = parser.add_subparsers(dest="cmd", help='Valid commands are: rpmb, preloader, boot2, memread, memwrite, keys')

    parser_rpmb = subparsers.add_parser("rpmb", help="Dump the rpmb")
    parser_rpmb.add_argument('--start', dest='start', type=str,
                        help='Start offset to dump')
    parser_rpmb.add_argument('--length', dest='length', type=str,
                        help='Max length to dump')
    parser_rpmb.add_argument('--reverse', dest='reverse', action="store_true",
                        help='Reverse byte order (example: rpmb command)')
    parser_rpmb.add_argument('--filename', dest='filename', type=str,
                        help='Read from / save to filename')

    parser_preloader = subparsers.add_parser("preloader", help="Dump the preloader")
    parser_preloader.add_argument('--start', dest='start', type=str,
                        help='Start offset to dump')
    parser_preloader.add_argument('--length', dest='length', type=str,
                        help='Max length to dump')
    parser_preloader.add_argument('--filename', dest='filename', type=str,
                        help='Read from / save to filename')

    parser_boot2 = subparsers.add_parser("boot2", help="Dump boot2")
    parser_boot2.add_argument('--start', dest='start', type=str,
                        help='Start offset to dump')
    parser_boot2.add_argument('--length', dest='length', type=str,
                        help='Max length to dump')
    parser_boot2.add_argument('--filename', dest='filename', type=str,
                        help='Read from / save to filename')

    parser_memread = subparsers.add_parser("memread", help="Read memory")
    parser_memread.add_argument(dest='start', type=str,
                        help='Start offset to dump')
    parser_memread.add_argument(dest='length', type=str,
                        help='Max length to dump')
    parser_memread.add_argument('--filename', dest='filename', type=str,
                        help='Save to filename')

    parser_memwrite = subparsers.add_parser("memwrite", help="Write memory")
    parser_memwrite.add_argument(dest='start', type=str,
                        help='Start offset to dump')
    parser_memwrite.add_argument('data', type=str,
                        help='Data to write [hexstring, dword or filename]')

    parser_reboot = subparsers.add_parser("reboot", help="Reboot device")

    parser_seccfg = subparsers.add_parser("seccfg", help="Generate seccfg")
    parser_seccfg.add_argument('flag', type=str,
                        help='Option for generating: unlock or lock')
    parser_seccfg.add_argument('--sw', dest='sw', action="store_true",
                        help='Option for generating: sw or hw')

    parser_keys = subparsers.add_parser("keys", help="Write memory")
    parser_keys.add_argument('--otp', dest='otp', type=str,
                        help='OTP for keys (dxcc,sej,gcpu)')
    parser_keys.add_argument('--mode', dest='mode', default=None, type=str,
                        help='keymode (dxcc,sej,gcpu)')
    args = parser.parse_args()
    cmd = args.cmd
    if cmd not in cmds:
        showcommands()
        exit(0)

    if not os.path.exists("logs"):
        os.mkdir("logs")
    st2 = Stage2(args)
    if st2.connect():
        if not st2.preinit():
            exit(1)

        if cmd == "rpmb":
            if args.filename is None:
                filename = os.path.join("logs", "rpmb")
            else:
                filename = args.filename
            start = getint(args.start)
            length = getint(args.length)
            st2.rpmb(start, length, filename, args.reverse)
        elif cmd == "preloader":
            if args.filename is None:
                filename = os.path.join("logs", "preloader")
            else:
                filename = args.filename
            start = getint(args.start)
            length = getint(args.length)
            st2.preloader(start, length, filename=filename)
        elif cmd == "boot2":
            if args.filename is None:
                filename = os.path.join("logs", "boot2")
            else:
                filename = args.filename
            start = getint(args.start)
            length = getint(args.length)
            st2.boot2(start, length, filename=filename)
        elif cmd == "memread":
            if args.start is None:
                print("Option --start is needed")
                exit(0)
            if args.length is None:
                print("Option --length is needed")
                exit(0)
            start = getint(args.start)
            length = getint(args.length)
            st2.memread(start, length, args.filename)
        elif cmd == "memwrite":
            if args.start is None:
                print("Option --start is needed")
                exit(0)
            if args.data is None:
                print("Option --data is needed")
                exit(0)
            start = getint(args.start)
            if os.path.exists(args.data):
                filename=args.data
                data=None
            else:
                if "0x" in args.data:
                    data=getint(args.data)
                else:
                    data=args.data
                filename=None
            if st2.memwrite(start, data, filename):
                print(f"Successfully wrote data to {hex(start)}.")
            else:
                print(f"Failed to write data to {hex(start)}.")
        elif cmd == "keys":
            keyinfo=""
            data=b""
            if st2.hwcrypto.meid_addr:
                meid = st2.memread(st2.hwcrypto.meid_addr, 16)
                keyinfo+=f"MEID: {hexlify(meid).decode('utf-8')}\n"
                with open(os.path.join("logs", "meid.txt"), "wb") as wf:
                    wf.write(hexlify(meid))
            if st2.hwcrypto.socid_addr:
                socid = st2.memread(st2.hwcrypto.socid_addr, 32)
                keyinfo += f"SOCID: {hexlify(socid).decode('utf-8')}\n"
                with open(os.path.join("logs", "socid.txt"), "wb") as wf:
                    wf.write(hexlify(socid))
            if st2.setup.sej_base or args.mode == "sej":
                data = meid
                # if not args.otp:
                #    print("Option --otp is needed")
                #    exit(0)
            if args.mode == "sej_aes_decrypt" or args.mode == "sej_aes_encrypt":
                if not args.data:
                    print("Option --data is needed")
                    exit(0)
                data = bytes.fromhex(args.data)
            # otp_hisense=bytes.fromhex("486973656E736500000000000000000000000000000000000000000000000000")
            # st2.jump(0x223449)
            keys, keyinfo=st2.keys(data=data, mode=args.mode, otp=args.otp)
            print(keyinfo)
            with open("keys.txt","w") as wf:
                wf.write(keyinfo)
                print("Wrote keys to keys.txt")
        elif cmd == "reboot":
            st2.reboot()
        elif cmd == "seccfg":
            if args.flag not in ["unlock","lock"]:
                print("Valid flags are: unlock, lock")
                sys.exit(1)
                """
                LKS_DEFAULT = 0x01
                LKS_MP_DEFAULT = 0x02
                LKS_UNLOCK = 0x03
                LKS_LOCK = 0x04
                LKS_VERIFIED = 0x05
                LKS_CUSTOM = 0x06
                """
                """
                LKCS_UNLOCK = 0x01
                LKCS_LOCK = 0x02
                """
                """
                SBOOT_RUNTIME_OFF = 0
                SBOOT_RUNTIME_ON  = 1
                """
            if args.flag=="unlock":
                lock_state = 3
                critical_lock_state = 1
            elif args.flag=="lock":
                lock_state = 1
                critical_lock_state = 0
            with open("seccfg.bin", "wb") as wf:
                seccfg_ver = 4
                seccfg_size = 0x3C                
                sboot_runtime = 0
                seccfg_data = pack("<IIIIIII", 0x4D4D4D4D, seccfg_ver, seccfg_size, lock_state,
                                   critical_lock_state, sboot_runtime, 0x45454545)
                dec_hash = hashlib.sha256(seccfg_data).digest()
                if args.sw:
                    enc_hash = st2.hwcrypto.sej.sej_sec_cfg_sw(dec_hash, True)
                else:
                    enc_hash = st2.hwcrypto.sej.sej_sec_cfg_hw(dec_hash,True)
                data = seccfg_data + enc_hash
                data += b"\x00" * (0x200 - len(data))
                wf.write(data)
                print("Successfully wrote seccfg to seccfg.bin. You need to write seccfg.bin to partition seccfg.")
    st2.close()

if __name__ == "__main__":
    main()
