Metadata-Version: 2.1
Name: mtkclient
Version: 1.4
Summary: Mediatek reverse engineering and flashing tools
Home-page: https://github.com/bkerler/mtkclient
Author: B. Kerler
Author-email: info@revskills.de
License: MIT License
Project-URL: Bug Tracker, https://github.com/bkerler/mtkclient/issues
Platform: UNKNOWN
Classifier: Programming Language :: Python :: 3
Classifier: License :: OSI Approved :: MIT License
Classifier: Operating System :: OS Independent
Requires-Python: >=3.7
Description-Content-Type: text/markdown
License-File: LICENSE

# mtkclient
Just some mtk tool for exploitation, reading/writing flash and doing crazy stuff. 
For windows, you need to install the stock mtk port and the usbdk driver (see instructions below).
For linux, a patched kernel is only needed when using old kamakiri (see Setup folder) (except for read/write flash).

Once the mtk script is running, boot into brom mode by powering off device, press and hold either
vol up + power or vol down + power and connect the phone. Once detected by the tool,
release the buttons.

## Credits
- kamakiri [xyzz]
- linecode exploit [chimera]
- Chaosmaster
- All contributors

## Installation

### Use Re LiveDVD (everything ready to go, based on Ubuntu):
[Download Re Live DVD V2](https://drive.google.com/file/d/1VUK0toC6I0jhJ4ZTFPREhSXFTkSe9_gl/view?usp=sharing)
User: livedvd, Password:livedvd


## Install

### Linux - (Ubuntu recommended, no patched kernel needed except for kamakiri)

#### Install python >=3.8, git and other deps

```
sudo apt install python3 git libusb1.0
```

#### Grab files 
```
git clone https://github.com/bkerler/mtkclient
cd mtkclient
pip3 install -r requirements.txt
python3 setup.py build
python3 setup.py install
```

#### Install rules
```
sudo usermod -a -G plugdev $USER
sudo usermod -a -G dialout $USER
sudo cp Setup/Linux/*.rules /etc/udev/rules.d
sudo udevadm control -R
```
Make sure to reboot after adding the user to dialout/plugdev.

---------------------------------------------------------------------------------------------------------------

### Windows

#### Install python + git
- Install python 3.9 and git
- If you install python from microsoft store, "python setup.py install" will fail, but that step isn't required.
- WIN+R ```cmd```

#### Grab files and install
```
git clone https://github.com/bkerler/mtkclient
cd mtkclient
pip3 install -r requirements.txt
```

#### Get latest UsbDk 64-Bit
- Install normal MTK Serial Port driver (or use default Windows COM Port one, make sure no exclamation is seen)
- Get usbdk installer (.msi) from [here](https://github.com/daynix/UsbDk/releases/) and install it
- Test on device connect using "UsbDkController -n" if you see a device with 0x0E8D 0x0003
- Works fine under Windows 10 and 11 :D

---------------------------------------------------------------------------------------------------------------
### Use kamakiri (optional, only needed for mt6260 or older)

- For linux (kamakiri attack), you need to recompile your linux kernel using this kernel patch :
```
sudo apt-get install build-essential libncurses-dev bison flex libssl-dev libelf-dev libdw-dev
git clone https://git.kernel.org/pub/scm/devel/pahole/pahole.git
cd pahole && mkdir build && cd build && cmake .. && make && sudo make install
sudo mv /usr/local/libdwarves* /usr/local/lib/ && sudo ldconfig
```

```
wget https://cdn.kernel.org/pub/linux/kernel/v5.x/linux-`uname -r`.tar.xz
tar xvf linux-`uname -r`.tar.xz
cd linux-`uname -r`
patch -p1 < ../Setup/kernelpatches/disable-usb-checks-5.10.patch
cp -v /boot/config-$(uname -r) .config
make menuconfig
make
sudo make modules_install 
sudo make install
```

- These aren't needed for current ubuntu (as make install will do, just for reference):

```
sudo update-initramfs -c -k `uname -r`
sudo update-grub
```

See Setup/kernels for ready-to-use kernel setups


- Reboot

```
sudo reboot
```


---------------------------------------------------------------------------------------------------------------

## Usage

### Root the phone (Tested with android 9 - 12)

1. Dump boot and vbmeta
```
python mtk r boot,vbmeta boot.img,vbmeta.img
```

2. Reboot the phone
```
python mtk reset
```

3. Download patched magisk for mtk:
Download (here)[https://raw.githubusercontent.com/vvb2060/magisk_files/44ca9ed38c29e22fa276698f6c03bc1168df2c10/app-release.apk]

4. Install on target phone
- you need to enable usb-debugging via Settings/About phone/Version, Tap 7x on build number
- Go to Settings/Additional settings/Developer options, enable "OEM unlock" and "USB Debugging"
- Install magisk apk
```
adb install app-release.apk
```
- accept auth rsa request on mobile screen of course to allow adb connection

5. Upload boot to /sdcard/Download
```
adb push boot.img /sdcard/Download
```

6. Start magisk, tap on Install, select boot.img from /sdcard/Download, then:
```
adb pull /sdcard/Download/[displayed magisk patched boot filename here]
mv [displayed magisk patched boot filename here] boot.patched
```

7. Do the steps needed in section "Unlock bootloader below"

8. Flash magisk-patched boot and empty vbmeta
```
python mtk w boot,vbmeta boot.patched,vbmeta.img.empty
```

9. Reboot the phone
```
python mtk reset
```

10. Disconnect usb cable and enjoy your rooted phone :)


### Unlock bootloader

1. Erase metadata and userdata (and md_udc if existing):
```
python mtk e metadata,userdata,md_udc
```

2. Unlock bootloader:
```
python mtk xflash seccfg unlock
```
for relocking use:
```
python mtk xflash seccfg lock
```

3. Reboot the phone:
```
python mtk reset
```

and disconnect usb cable to let the phone reboot.

If you are getting a dm-verity error on Android 11, just press the power button,
then the device should boot and show a yellow warning about unlocked bootloader and
then the device should boot within 5 seconds.


### Read flash

Dump boot partition to filename boot.bin via preloader

```
python mtk r boot boot.bin
```

Dump boot partition to filename boot.bin via bootrom

```
python mtk r boot boot.bin [--preloader=Loader/Preloader/your_device_preloader.bin]
```


Read full flash to filename flash.bin (use --preloader for brom)

```
python mtk rf flash.bin
```

Dump all partitions to directory "out". (use --preloader for brom)

```
python mtk rl out
```

Show gpt (use --preloader for brom)

```
python mtk printgpt
```


### Write flash
(use --preloader for brom)

Write filename boot.bin to boot partition

```
python mtk w boot boot.bin
```

Write filename flash.bin as full flash (currently only works in da mode)

```
python mtk wf flash.bin
```

Write all files in directory "out" to the flash partitions

```
python mtk wl out
```

### Erase flash

Erase boot partition
```
python mtk e boot
```

Erase boot sectors
```
python mtk es boot [sector count]
```

### XFlash commands (only available via XFlash da, not legacy da for now):

Peek memory
```
python mtk xflash peek [addr in hex] [length in hex] [optional: -filename filename.bin for reading to file]
```

Poke memory
```
python mtk xflash peek [addr in hex] [data as hexstring or -filename for reading from file]
```

Read rpmb
```
python mtk xflash rpmb r [will read to rpmb.bin]
```

Write rpmb [Dangerous and may not work as it's not tested !]
```
python mtk xflash rpmb w filename
```

Generate and display rpmb1-3 key
```
python mtk xflash generatekeys
```

Unlock / Lock bootloader
```
python mtk xflash seccfg [lock or unlock]
```

---------------------------------------------------------------------------------------------------------------

### Bypass SLA, DAA and SBC (using generic_patcher_payload)
`` 
python mtk payload
`` 
If you want to use SP Flash tool afterwards, make sure you select "UART" in the settings, not "USB".

### Dump preloader
- Device has to be in bootrom mode and preloader has to be intact on the device
```
python mtk dumppreloader [--ptype=["amonet","kamakiri","kamakiri2","hashimoto"]] [--filename=preloader.bin]
```

### Dump brom
- Device has to be in bootrom mode, or da mode has to be crashed to enter damode
- if no option is given, either kamakiri or da will be used (da for insecure targets)
- if "kamakiri" is used as an option, kamakiri is enforced
- Valid options are : "kamakiri" (via usb_ctrl_handler attack), "amonet" (via gcpu)
  and "hashimoto" (via cqdma)

```
python mtk dumpbrom --ptype=["amonet","kamakiri","hashimoto"] [--filename=brom.bin]
```

For to dump unknown bootroms, use brute option :
```
python mtk brute
```
If it's successful, please add an issue over here and append the bootrom in order to add full support.

---------------------------------------------------------------------------------------------------------------

### Crash da in order to enter brom

```
python mtk crash [--vid=vid] [--pid=pid] [--interface=interface]
```

### Read memory using patched preloader
- Boot in Brom or crash to Brom
```
python mtk peek [addr] [length] --preloader=patched_preloader.bin
```

### Run custom payload

```
python mtk payload --payload=payload.bin [--var1=var1] [--wdt=wdt] [--uartaddr=addr] [--da_addr=addr] [--brom_addr=addr]
```

---------------------------------------------------------------------------------------------------------------
## Stage2 usage
### Run python mtk stage (brom) or mtk plstage (preloader)

#### Run stage2 in bootrom
`` 
python mtk stage
`` 

#### Run stage2 in preloader
`` 
python mtk plstage
`` 

#### Run stage2 plstage in bootrom
- Boot in Brom or crash to Brom
```
python mtk plstage --preloader=preloader.bin
```

### Use stage2 tool


### Leave stage2 and reboot
`` 
python stage2 reboot
`` 

### Read rpmb in stage2 mode
`` 
python stage2 rpmb
`` 

### Read preloader in stage2 mode
`` 
python stage2 preloader
`` 

### Read memory as hex data in stage2 mode
`` 
python stage2 memread [start addr] [length]
`` 

### Read memory to file in stage2 mode
`` 
python stage2 memread [start addr] [length] --filename filename.bin
`` 

### Write hex data to memory in stage2 mode
`` 
python stage2 memwrite [start addr] --data [data as hexstring]
`` 

### Write memory from file in stage2 mode
`` 
python stage2 memwrite [start addr] --filename filename.bin
`` 

### Extract keys
`` 
python stage2 keys --mode [sej, dxcc]
`` 
For dxcc, you need to use plstage instead of stage

---------------------------------------------------------------------

### I have issues ....... please send logs and full console details !

- Run the mtk tool with --debugmode. Log will be written to log.txt (hopefully)

## Rules / Infos

### Chip details / configs
- Go to config/brom_config.py
- Unknown usb vid/pids for autodetection go to config/usb_ids.py


